From f7b61dd11c404f5268fcf651744388c10f47d974 Mon Sep 17 00:00:00 2001
From: Huang Qi <huangqi3@xiaomi.com>
Date: Thu, 28 Jan 2021 13:29:25 +0800
Subject: [PATCH 06/21] LTP: Re-init static variable to avoid errors during
 multiple runs

MIRTOS-361

Signed-off-by: Huang Qi <huangqi3@xiaomi.com>
Change-Id: I81fb72b33a3381dfe18c0193e56bcd3d67a3a5eb
---
 .../conformance/interfaces/pthread_cond_signal/2-1.c           | 3 +++
 .../conformance/interfaces/pthread_cond_signal/4-1.c           | 3 +++
 2 files changed, 6 insertions(+)

diff --git a/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/2-1.c b/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/2-1.c
index ff62336c9..c00cb4731 100644
--- a/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/2-1.c
+++ b/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/2-1.c
@@ -101,6 +101,9 @@ int main(void)
 	struct sigaction act;
 	pthread_mutexattr_t ma;
 
+	waken_num = 0;
+	start_num = 0;
+
 	if (pthread_mutexattr_init(&ma) != 0) {
 		fprintf(stderr, "Fail to initialize mutex attribute\n");
 		return PTS_UNRESOLVED;
diff --git a/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/4-1.c b/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/4-1.c
index 36dc91ec9..bbb7acfcf 100644
--- a/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/4-1.c
+++ b/testcases/open_posix_testsuite/conformance/interfaces/pthread_cond_signal/4-1.c
@@ -79,6 +79,9 @@ int main(void)
 	int i, rc;
 	struct sigaction act;
 
+	waken_num = 0;
+	start_num = 0;
+
 	if (pthread_mutex_init(&td.mutex, NULL) != 0) {
 		fprintf(stderr, "Fail to initialize mutex\n");
 		return PTS_UNRESOLVED;
-- 
2.40.1

