############################################################################
# configs/ez80f910200zco/poll/defconfig
#
#   Copyright (C) 2009-2010 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################
#
# Architecture selection
#
CONFIG_ARCH="z80"
CONFIG_ARCH_Z80=y
CONFIG_ARCH_CHIP="ez80"
CONFIG_ARCH_CHIP_EZ80=y
CONFIG_ARCH_CHIP_EZ80F91=y
CONFIG_ARCH_CHIP_EZ80F92=n
CONFIG_ARCH_CHIP_EZ80F93=n
CONFIG_ARCH_BOARD="ez80f910200zco"
CONFIG_ARCH_BOARD_EZ80F910200ZCO=y
CONFIG_ARCH_NOINTC=n
CONFIG_ARCH_IRQPRIO=n
CONFIG_BOARD_LOOPSPERMSEC=1250
CONFIG_ENDIAN_BIG=n
CONFIG_DRAM_SIZE=65536
CONFIG_ARCH_LEDS=y
CONFIG_ARCH_BUTTONS=n
CONFIG_ARCH_TIMERHOOK=y
CONFIG_ARCH_STACKDUMP=n

#
# eZ80 specific device driver settings
#
CONFIG_EZ80_UART0=y
CONFIG_EZ80_UART1=n
CONFIG_UART0_SERIAL_CONSOLE=y
CONFIG_UART1_SERIAL_CONSOLE=n
CONFIG_UART0_TXBUFSIZE=0
CONFIG_UART1_TXBUFSIZE=0
CONFIG_UART0_RXBUFSIZE=0
CONFIG_UART1_RXBUFSIZE=0
CONFIG_UART0_BAUD=57600
CONFIG_UART1_BAUD=57600
CONFIG_UART0_BITS=0
CONFIG_UART1_BITS=0
CONFIG_UART0_PARITY=0
CONFIG_UART1_PARITY=0
CONFIG_UART0_2STOP=0
CONFIG_UART1_2STOP=0

#
# ez80 EMAC
#
CONFIG_EZ80_EMAC=y
CONFIG_EZ80_FIAD=0x1f
CONFIG_EZ80_PHYAM79C874=y
CONFIG_EZ80_PHYCONFIG=1
CONFIG_EZ80_RAMADDR=0xf7c000
CONFIG_EZ80_PKTBUFSIZE=64
CONFIG_EZ80_NTXPKTBUFS=64
CONFIG_EZ80_NRXPKTBUFS=64
CONFIG_EZ80_PKTBUFSIZE=64
CONFIG_EZ80_MDCDIV=0
CONFIG_EZ80_TXPOLLTIMERMS=10
CONFIG_ARCH_MCFILTER=n

#
# General build options
#
CONFIG_RRLOAD_BINARY=n
CONFIG_INTELHEX_BINARY=n
CONFIG_MOTOROLA_SREC=n
CONFIG_RAW_BINARY=n

#
# General OS setup
#
CONFIG_USER_ENTRYPOINT="poll_main"
CONFIG_DEBUG=y
CONFIG_DEBUG_VERBOSE=n
CONFIG_DEBUG_SYMBOLS=n
CONFIG_DEBUG_NET=n
CONFIG_MM_REGIONS=1
CONFIG_ARCH_LOWPUTC=y
CONFIG_RR_INTERVAL=200
CONFIG_SCHED_INSTRUMENTATION=n
CONFIG_TASK_NAME_SIZE=0
CONFIG_START_YEAR=2009
CONFIG_START_MONTH=3
CONFIG_START_DAY=14
CONFIG_JULIAN_TIME=n
CONFIG_HAVE_LOWSERIALINIT=y
CONFIG_DEV_CONSOLE=y
CONFIG_DEV_LOWCONSOLE=y
CONFIG_MUTEX_TYPES=n
CONFIG_PRIORITY_INHERITANCE=n
CONFIG_SEM_PREALLOCHOLDERS=0
CONFIG_SEM_NNESTPRIO=0
CONFIG_FDCLONE_DISABLE=n
CONFIG_FDCLONE_STDIO=n
CONFIG_SDCLONE_DISABLE=y

#
# The following can be used to disable categories of
# APIs supported by the OS.  If the compiler supports
# weak functions, then it should not be necessary to
# disable functions unless you want to restrict usage
# of those APIs.
#
# There are certain dependency relationships in these
# features.
#
# o mq_notify logic depends on signals to awaken tasks
#   waiting for queues to become full or empty.
# o pthread_condtimedwait() depends on signals to wake
#   up waiting tasks.
#
CONFIG_DISABLE_CLOCK=n
CONFIG_DISABLE_POSIX_TIMERS=n
CONFIG_DISABLE_PTHREAD=n
CONFIG_DISABLE_SIGNALS=n
CONFIG_DISABLE_MQUEUE=y
CONFIG_DISABLE_MOUNTPOINT=y
CONFIG_DISABLE_ENVIRON=y
CONFIG_DISABLE_POLL=n

#
# Misc libc settings
#
CONFIG_NOPRINTF_FIELDWIDTH=n

#
# Allow for architecture optimized implementations
#
# The architecture can provide optimized versions of the
# following to improve sysem performance
#
CONFIG_ARCH_MEMCPY=n
CONFIG_ARCH_MEMCMP=n
CONFIG_ARCH_MEMMOVE=n
CONFIG_ARCH_MEMSET=n
CONFIG_ARCH_STRCMP=n
CONFIG_ARCH_STRCPY=n
CONFIG_ARCH_STRNCPY=n
CONFIG_ARCH_STRLEN=n
CONFIG_ARCH_STRNLEN=n
CONFIG_ARCH_BZERO=n

#
# Sizes of configurable things (0 disables)
#
CONFIG_MAX_TASKS=8
CONFIG_MAX_TASK_ARGS=4
CONFIG_NPTHREAD_KEYS=0
CONFIG_NFILE_DESCRIPTORS=8
CONFIG_NFILE_STREAMS=8
CONFIG_NAME_MAX=32
CONFIG_STDIO_BUFFER_SIZE=0
CONFIG_NUNGET_CHARS=0
CONFIG_PREALLOC_MQ_MSGS=0
CONFIG_MQ_MAXMSGSIZE=0
CONFIG_MAX_WDOGPARMS=4
CONFIG_PREALLOC_WDOGS=8
CONFIG_PREALLOC_TIMERS=8

#
# Framebuffer driver options
CONFIG_FB_CMAP=n
CONFIG_FB_HWCURSOR=n
CONFIG_FB_HWCURSORIMAGE=n
#CONFIG_FB_HWCURSORSIZE
#CONFIG_FB_TRANSPARENCY

#
# Filesystem configuration
#
CONFIG_FS_FAT=n
CONFIG_FS_ROMFS=n

#
# Maintain legacy build behavior (revisit)
#

CONFIG_MMCSD=y
CONFIG_MMCSD_SPI=y
CONFIG_MTD=y

#
# SPI-based MMC/SD driver
#
CONFIG_MMCSD_NSLOTS=1
CONFIG_MMCSD_READONLY=n

#
# TCP/IP and UDP support via uIP
#
CONFIG_NET=y
CONFIG_NET_IPv6=n
CONFIG_NSOCKET_DESCRIPTORS=8
CONFIG_NET_SOCKOPTS=y
CONFIG_NET_BUFSIZE=420
CONFIG_NET_TCP=y
CONFIG_NET_TCP_CONNS=8
CONFIG_NET_NTCP_READAHEAD_BUFFERS=8
CONFIG_NET_TCPBACKLOG=y
CONFIG_NET_MAX_LISTENPORTS=8
CONFIG_NET_UDP=n
CONFIG_NET_UDP_CHECKSUMS=y
#CONFIG_NET_UDP_CONNS=10
CONFIG_NET_ICMP=y
CONFIG_NET_ICMP_PING=n
#CONFIG_NET_PINGADDRCONF=0
CONFIG_NET_STATISTICS=n
#CONFIG_NET_RECEIVE_WINDOW=
#CONFIG_NET_ARPTAB_SIZE=8
CONFIG_NET_BROADCAST=n

#
# UIP Network Utilities
#
CONFIG_NET_DHCP_LIGHT=n
CONFIG_NET_RESOLV_ENTRIES=4

#
# USB Device Configuration
#
CONFIG_USBDEV=n
CONFIG_USBDEV_ISOCHRONOUS=n
CONFIG_USBDEV_DUALSPEED=n
CONFIG_USBDEV_SELFPOWERED=y
CONFIG_USBDEV_REMOTEWAKEUP=n
CONFIG_USBDEV_MAXPOWER=100
CONFIG_USBDEV_TRACE=n
CONFIG_USBDEV_TRACE_NRECORDS=128

#
# USB Serial Device Configuration
#
CONFIG_PL2303=n
CONFIG_PL2303_EPINTIN=1
CONFIG_PL2303_EPBULKOUT=2
CONFIG_PL2303_EPBULKIN=5
CONFIG_PL2303_NWRREQS=4
CONFIG_PL2303_NRDREQS=4
CONFIG_PL2303_VENDORID=0x067b
CONFIG_PL2303_PRODUCTID=0x2303
CONFIG_PL2303_VENDORSTR="Nuttx"
CONFIG_PL2303_PRODUCTSTR="USBdev Serial"
CONFIG_PL2303_RXBUFSIZE=512
CONFIG_PL2303_TXBUFSIZE=512

#
# USB Storage Device Configuration
#
CONFIG_USBMSC=n
CONFIG_USBMSC_EP0MAXPACKET=64
CONFIG_USBMSC_EPBULKOUT=2
CONFIG_USBMSC_EPBULKIN=5
CONFIG_USBMSC_NRDREQS=2
CONFIG_USBMSC_NWRREQS=2
CONFIG_USBMSC_BULKINREQLEN=256
CONFIG_USBMSC_BULKOUTREQLEN=256
CONFIG_USBMSC_VENDORID=0x584e
CONFIG_USBMSC_VENDORSTR="NuttX"
CONFIG_USBMSC_PRODUCTID=0x5342
CONFIG_USBMSC_PRODUCTSTR="USBdev Storage"
CONFIG_USBMSC_VERSIONNO=0x0399
CONFIG_USBMSC_REMOVABLE=y

#
CONFIG_NX=n
CONFIG_NX_MULTIUSER=n
CONFIG_NX_NPLANES=1
CONFIG_NX_DISABLE_1BPP=y
CONFIG_NX_DISABLE_2BPP=y
CONFIG_NX_DISABLE_4BPP=y
CONFIG_NX_DISABLE_8BPP=n
CONFIG_NX_DISABLE_16BPP=y
CONFIG_NX_DISABLE_24BPP=y
CONFIG_NX_DISABLE_32BPP=y
CONFIG_NX_PACKEDMSFIRST=n
CONFIG_NX_MOUSE=y
CONFIG_NX_KBD=y
#CONFIG_NXTK_BORDERWIDTH=4
#CONFIG_NXTK_BORDERCOLOR1
#CONFIG_NXTK_BORDERCOLOR2
CONFIG_NXTK_AUTORAISE=n
CONFIG_NXFONT_SANS23X27=y
CONFIG_NXFONTS_CHARBITS=7
CONFIG_NX_BLOCKING=y
CONFIG_NX_MXSERVERMSGS=32
CONFIG_NX_MXCLIENTMSGS=16

#
# Settings for examples/poll
CONFIG_EXAMPLES_POLL_NOMAC=y
CONFIG_EXAMPLES_POLL_IPADDR=0x0a000002
CONFIG_EXAMPLES_POLL_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_POLL_NETMASK=0xffffff00

#
# Settings for examples/uip
CONFIG_EXAMPLES_UIP_IPADDR=0x0a000002
CONFIG_EXAMPLES_UIP_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_UIP_NETMASK=0xffffff00
CONFIG_EXAMPLES_UIP_DHCPC=n

#
# Settings for examples/nettest
#
CONFIG_EXAMPLES_NETTEST_SERVER=n
CONFIG_EXAMPLES_NETTEST_PERFORMANCE=n
CONFIG_EXAMPLES_NETTEST_NOMAC=y
CONFIG_EXAMPLES_NETTEST_IPADDR=0x0a000002
CONFIG_EXAMPLES_NETTEST_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_NETTEST_NETMASK=0xffffff00
CONFIG_EXAMPLES_NETTEST_CLIENTIP=0x0a000001

#
# Settings for examples/ostest
CONFIG_EXAMPLES_OSTEST_LOOPS=1
CONFIG_EXAMPLES_OSTEST_STACKSIZE=2048
CONFIG_EXAMPLES_OSTEST_NBARRIER_THREADS=3

#
# Settings for apps/nshlib
#
CONFIG_NSH_FILEIOSIZE=512
CONFIG_NSH_STRERROR=n
CONFIG_NSH_LINELEN=64
CONFIG_NSH_NESTDEPTH=3
CONFIG_NSH_DISABLESCRIPT=n
CONFIG_NSH_DISABLEBG=n
CONFIG_NSH_ROMFSETC=n
CONFIG_NSH_CONSOLE=y
CONFIG_NSH_TELNET=n
CONFIG_NSH_IOBUFFER_SIZE=512
CONFIG_NSH_DHCPC=n
CONFIG_NSH_NOMAC=y
CONFIG_NSH_IPADDR=0x0a000002
CONFIG_NSH_DRIPADDR=0x0a000001
CONFIG_NSH_NETMASK=0xffffff00
CONFIG_NSH_ROMFSMOUNTPT="/etc"
CONFIG_NSH_INITSCRIPT="init.d/rcS"
CONFIG_NSH_ROMFSDEVNO=0
CONFIG_NSH_ROMFSSECTSIZE=64
CONFIG_NSH_FATDEVNO=1
CONFIG_NSH_FATSECTSIZE=512
CONFIG_NSH_FATNSECTORS=1024
CONFIG_NSH_FATMOUNTPT="/tmp"

#
# Architecture-specific NSH options
CONFIG_NSH_MMCSDSPIPORTNO=1
CONFIG_NSH_MMCSDSLOTNO=0
CONFIG_NSH_MMCSDMINOR=0

#
# Settings for examples/nx
#
CONFIG_EXAMPLES_NX_VPLANE=0
#CONFIG_EXAMPLES_NX_BGCOLOR
#CONFIG_EXAMPLES_NX_COLOR1
#CONFIG_EXAMPLES_NX_COLOR2
#CONFIG_EXAMPLES_NX_TBCOLOR
#CONFIG_EXAMPLES_NX_FONTCOLOR
CONFIG_EXAMPLES_NX_BPP=CONFIG_SIM_FBBPP
CONFIG_EXAMPLES_NX_RAWWINDOWS=n
CONFIG_EXAMPLES_NX_STACKSIZE=8192
CONFIG_EXAMPLES_NX_CLIENTPRIO=80
CONFIG_EXAMPLES_NX_SERVERPRIO=120
CONFIG_EXAMPLES_NX_NOTIFYSIGNO=4

#
# Settings for examples/mount
CONFIG_EXAMPLES_MOUNT_DEVNAME="/dev/ram0"
#CONFIG_EXAMPLES_MOUNT_NSECTORS=2048
#CONFIG_EXAMPLES_MOUNT_SECTORSIZE=512
#CONFIG_EXAMPLES_MOUNT_RAMDEVNO=1

#
# Settings for examples/wget
#
CONFIG_EXAMPLES_WGET_URL="http://www.nuttx.org/index.html"
CONFIG_EXAMPLES_WGET_NOMAC=y
CONFIG_EXAMPLES_WGET_IPADDR=0x0a000002
CONFIG_EXAMPLES_WGET_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_WGET_NETMASK=0xffffff00

#
# Stack and heap information
#
CONFIG_BOOT_RUNFROMFLASH=n
CONFIG_BOOT_COPYTORAM=n
CONFIG_CUSTOM_STACK=n
CONFIG_IDLETHREAD_STACKSIZE=1024
CONFIG_USERMAIN_STACKSIZE=1024
CONFIG_PTHREAD_STACK_MIN=256
CONFIG_PTHREAD_STACK_DEFAULT=1024
