############################################################################
# configs/stm3240g-eval/nsh/defconfig
#
#   Copyright (C) 2011-2012 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################
#
# Architecture Selection
#
CONFIG_ARCH="arm"
CONFIG_ARCH_ARM=y
CONFIG_ARCH_CORTEXM4=y
CONFIG_ARCH_CHIP="stm32"
CONFIG_ARCH_CHIP_STM32F407IG=y
CONFIG_ARCH_BOARD="stm3240g-eval"
CONFIG_ARCH_BOARD_STM3240G_EVAL=y
CONFIG_BOARD_LOOPSPERMSEC=16717
CONFIG_DRAM_SIZE=196608
CONFIG_DRAM_START=0x20000000
CONFIG_ARCH_IRQPRIO=y
CONFIG_ARCH_FPU=n
CONFIG_ARCH_INTERRUPTSTACK=0
CONFIG_ARCH_STACKDUMP=y
CONFIG_ARCH_BOOTLOADER=n
CONFIG_ARCH_LEDS=y
CONFIG_ARCH_BUTTONS=n
CONFIG_ARCH_CALIBRATION=n
CONFIG_ARCH_DMA=n

#
# Identify toolchain and linker options
#
CONFIG_STM32_CODESOURCERYW=y
CONFIG_STM32_CODESOURCERYL=n
CONFIG_STM32_ATOLLIC_LITE=n
CONFIG_STM32_ATOLLIC_PRO=n
CONFIG_STM32_DEVKITARM=n
CONFIG_STM32_RAISONANCE=n
CONFIG_STM32_BUILDROOT=n

#
# JTAG Enable settings (by default JTAG-DP and SW-DP are disabled):
#
CONFIG_STM32_JTAG_FULL_ENABLE=y
CONFIG_STM32_JTAG_NOJNTRST_ENABLE=n
CONFIG_STM32_JTAG_SW_ENABLE=n

#
# On-chip CCM SRAM configuration
#

#
# On-board FSMC SRAM configuration
#
CONFIG_STM32_FSMC_SRAM=y
CONFIG_HEAP2_BASE=0x64000000
CONFIG_HEAP2_SIZE=2097152
  
#
# Individual subsystems can be enabled:
#
# AHB1:
CONFIG_STM32_CRC=n
CONFIG_STM32_BKPSRAM=n
CONFIG_STM32_CCMDATARAM=n
CONFIG_STM32_DMA1=n
CONFIG_STM32_DMA2=n
CONFIG_STM32_ETHMAC=y
CONFIG_STM32_OTGHS=n
# AHB2:
CONFIG_STM32_DCMI=n
CONFIG_STM32_CRYP=n
CONFIG_STM32_HASH=n
CONFIG_STM32_RNG=y
CONFIG_STM32_OTGFS=n
# AHB3:
CONFIG_STM32_FSMC=n
# APB1:
CONFIG_STM32_TIM2=n
CONFIG_STM32_TIM3=n
CONFIG_STM32_TIM4=n
CONFIG_STM32_TIM5=n
CONFIG_STM32_TIM6=n
CONFIG_STM32_TIM7=n
CONFIG_STM32_TIM12=n
CONFIG_STM32_TIM13=n
CONFIG_STM32_TIM14=n
CONFIG_STM32_WWDG=n
CONFIG_STM32_IWDG=n
CONFIG_STM32_SPI2=n
CONFIG_STM32_SPI3=n
CONFIG_STM32_USART2=n
CONFIG_STM32_USART3=y
CONFIG_STM32_UART4=n
CONFIG_STM32_UART5=n
CONFIG_STM32_I2C1=y
CONFIG_STM32_I2C2=n
CONFIG_STM32_I2C3=n
CONFIG_STM32_CAN1=n
CONFIG_STM32_CAN2=n
CONFIG_STM32_DAC=n
CONFIG_STM32_PWR=y
# APB2:
CONFIG_STM32_TIM1=n
CONFIG_STM32_TIM8=n
CONFIG_STM32_USART1=n
CONFIG_STM32_USART6=n
CONFIG_STM32_ADC1=n
CONFIG_STM32_ADC2=n
CONFIG_STM32_ADC3=n
CONFIG_STM32_SDIO=n
CONFIG_STM32_SPI1=n
CONFIG_STM32_SYSCFG=y
CONFIG_STM32_TIM9=n
CONFIG_STM32_TIM10=n
CONFIG_STM32_TIM11=n

#
# STM32F40xxx specific serial device driver settings
#
CONFIG_USART1_SERIAL_CONSOLE=n
CONFIG_USART2_SERIAL_CONSOLE=n
CONFIG_USART3_SERIAL_CONSOLE=y
CONFIG_UART4_SERIAL_CONSOLE=n
CONFIG_UART5_SERIAL_CONSOLE=n

CONFIG_USART1_TXBUFSIZE=128
CONFIG_USART2_TXBUFSIZE=128
CONFIG_USART3_TXBUFSIZE=128
CONFIG_UART4_TXBUFSIZE=128
CONFIG_UART5_TXBUFSIZE=128

CONFIG_USART1_RXBUFSIZE=128
CONFIG_USART2_RXBUFSIZE=128
CONFIG_USART3_RXBUFSIZE=128
CONFIG_UART4_RXBUFSIZE=128
CONFIG_UART5_RXBUFSIZE=128

CONFIG_USART1_BAUD=115200
CONFIG_USART2_BAUD=115200
CONFIG_USART3_BAUD=115200
CONFIG_UART4_BAUD=115200
CONFIG_UART5_BAUD=115200

CONFIG_USART1_BITS=8
CONFIG_USART2_BITS=8
CONFIG_USART3_BITS=8
CONFIG_UART4_BITS=8
CONFIG_UART5_BITS=8

CONFIG_USART1_PARITY=0
CONFIG_USART2_PARITY=0
CONFIG_USART3_PARITY=0
CONFIG_UART4_PARITY=0
CONFIG_UART5_PARITY=0

CONFIG_USART1_2STOP=0
CONFIG_USART2_2STOP=0
CONFIG_USART3_2STOP=0
CONFIG_UART4_2STOP=0
CONFIG_UART5_2STOP=0

#
# STM32F40xxx specific CAN device driver settings
#
CONFIG_CAN=n
CONFIG_CAN_EXTID=n
#CONFIG_CAN_FIFOSIZE
#CONFIG_CAN_NPENDINGRTR
CONFIG_CAN_LOOPBACK=n
CONFIG_CAN1_BAUD=700000
CONFIG_CAN2_BAUD=700000

#
# STM32F40xxx Ethernet device driver settings
#
CONFIG_STM32_PHYADDR=1
CONFIG_STM32_MII=y
CONFIG_STM32_MII_MCO1=y
CONFIG_STM32_MII_MCO2=n
CONFIG_STM32_RMII=n
CONFIG_STM32_AUTONEG=y
#CONFIG_STM32_ETHFD
#CONFIG_STM32_ETH100MB
CONFIG_STM32_PHYSR=16
CONFIG_STM32_PHYSR_SPEED=0x0002
CONFIG_STM32_PHYSR_100MBPS=0x0000
CONFIG_STM32_PHYSR_MODE=0x0004
CONFIG_STM32_PHYSR_FULLDUPLEX=0x0004
CONFIG_STM32_ETH_PTP=n
CONFIG_STM32_ETHMAC_REGDEBUG=n

#
# I2C configuration
#
CONFIG_I2C=y
CONFIG_I2C_POLLED=y
CONFIG_I2C_TRANSFER=y
CONFIG_I2C_TRACE=n

#
# ADC configuration
#
# Enable ADC driver support.  The STM3240G-EVAL has a 10 Kohm potentiometer
# RV1 connected to PF9 of STM32F407IGH6 on the board: TIM14_CH1/ SMC_CD/ADC3_IN7
#
CONFIG_ADC=n
#CONFIG_STM32_TIM1_ADC=y
CONFIG_STM32_TIM1_ADC3=y
CONFIG_STM32_ADC3_SAMPLE_FREQUENCY=100

#
# PWM configuration
#
# The STM3240G-Eval has no real on-board PWM devices, but the board can be configured to output
# a pulse train using several options (see board.h).  Here the default setup is for TIM8, CH4.
# Don't forget to enable CONFIG_PWM and CONFIG_STM32_TIM8.
#
CONFIG_PWM=n
CONFIG_PWM_PULSECOUNT=y
CONFIG_STM32_TIM8_PWM=y
CONFIG_STM32_TIM8_CHANNEL=4

#
# General build options
#
CONFIG_RRLOAD_BINARY=n
CONFIG_INTELHEX_BINARY=y
CONFIG_MOTOROLA_SREC=n
CONFIG_RAW_BINARY=n

#
# General OS setup
#
CONFIG_USER_ENTRYPOINT="nsh_main"
CONFIG_DEBUG=n
CONFIG_DEBUG_VERBOSE=n
CONFIG_DEBUG_SYMBOLS=n
CONFIG_DEBUG_FS=n
CONFIG_DEBUG_GRAPHICS=n
CONFIG_DEBUG_LCD=n
CONFIG_DEBUG_USB=n
CONFIG_DEBUG_NET=n
CONFIG_DEBUG_RTC=n
CONFIG_DEBUG_ANALOG=n
CONFIG_DEBUG_PWM=n
CONFIG_DEBUG_CAN=n
CONFIG_DEBUG_I2C=n
CONFIG_DEBUG_INPUT=n

CONFIG_HAVE_CXX=y
CONFIG_HAVE_CXXINITIALIZE=y
CONFIG_MM_REGIONS=2
CONFIG_ARCH_LOWPUTC=y
CONFIG_RR_INTERVAL=200
CONFIG_SCHED_INSTRUMENTATION=n
CONFIG_TASK_NAME_SIZE=0
CONFIG_START_YEAR=2011
CONFIG_START_MONTH=12
CONFIG_START_DAY=6
CONFIG_GREGORIAN_TIME=n
CONFIG_JULIAN_TIME=n
CONFIG_DEV_CONSOLE=y
CONFIG_DEV_LOWCONSOLE=n
CONFIG_MUTEX_TYPES=n
CONFIG_PRIORITY_INHERITANCE=n
CONFIG_SEM_PREALLOCHOLDERS=0
CONFIG_SEM_NNESTPRIO=0
CONFIG_FDCLONE_DISABLE=n
CONFIG_FDCLONE_STDIO=n
CONFIG_SDCLONE_DISABLE=y
CONFIG_SCHED_WORKQUEUE=n
CONFIG_SCHED_WORKPRIORITY=192
CONFIG_SCHED_WORKPERIOD=50000
CONFIG_SCHED_WORKSTACKSIZE=2048
CONFIG_SIG_SIGWORK=17
CONFIG_SCHED_WAITPID=y
CONFIG_SCHED_ATEXIT=n
CONFIG_DEV_RANDOM=y

#
# System Logging
#

CONFIG_SYSLOG=n
CONFIG_RAMLOG=n
CONFIG_RAMLOG_CONSOLE=n
CONFIG_RAMLOG_SYSLOG=n
#CONFIG_RAMLOG_NPOLLWAITERS
#CONFIG_RAMLOG_CONSOLE_BUFSIZE

#
# Settings for NXFLAT
#
CONFIG_NXFLAT=n
CONFIG_NXFLAT_DUMPBUFFER=n
CONFIG_SYMTAB_ORDEREDBYNAME=y

#
# The following can be used to disable categories of
# APIs supported by the OS.  If the compiler supports
# weak functions, then it should not be necessary to
# disable functions unless you want to restrict usage
# of those APIs.
#
# There are certain dependency relationships in these
# features.
#
# o mq_notify logic depends on signals to awaken tasks
#   waiting for queues to become full or empty.
# o pthread_condtimedwait() depends on signals to wake
#   up waiting tasks.
#
CONFIG_DISABLE_CLOCK=n
CONFIG_DISABLE_POSIX_TIMERS=n
CONFIG_DISABLE_PTHREAD=n
CONFIG_DISABLE_SIGNALS=n
CONFIG_DISABLE_MQUEUE=n
CONFIG_DISABLE_MOUNTPOINT=n
CONFIG_DISABLE_ENVIRON=n
CONFIG_DISABLE_POLL=y

#
# Misc libc settings
#
CONFIG_NOPRINTF_FIELDWIDTH=n

#
# Allow for architecture optimized implementations
#
# The architecture can provide optimized versions of the
# following to improve system performance
#
CONFIG_ARCH_MEMCPY=n
CONFIG_ARCH_MEMCMP=n
CONFIG_ARCH_MEMMOVE=n
CONFIG_ARCH_MEMSET=n
CONFIG_ARCH_STRCMP=n
CONFIG_ARCH_STRCPY=n
CONFIG_ARCH_STRNCPY=n
CONFIG_ARCH_STRLEN=n
CONFIG_ARCH_STRNLEN=n
CONFIG_ARCH_BZERO=n

#
# Sizes of configurable things (0 disables)
#
CONFIG_MAX_TASKS=16
CONFIG_MAX_TASK_ARGS=4
CONFIG_NPTHREAD_KEYS=4
CONFIG_NFILE_DESCRIPTORS=8
CONFIG_NFILE_STREAMS=8
CONFIG_NAME_MAX=32
CONFIG_STDIO_BUFFER_SIZE=64
CONFIG_STDIO_LINEBUFFER=y
CONFIG_NUNGET_CHARS=2
CONFIG_PREALLOC_MQ_MSGS=4
CONFIG_MQ_MAXMSGSIZE=32
CONFIG_MAX_WDOGPARMS=2
CONFIG_PREALLOC_WDOGS=8
CONFIG_PREALLOC_TIMERS=4

#
# Framebuffer driver options
#
CONFIG_FB_CMAP=n
CONFIG_FB_HWCURSOR=n
CONFIG_FB_HWCURSORIMAGE=n
#CONFIG_FB_HWCURSORSIZE
#CONFIG_FB_TRANSPARENCY

#
# Filesystem configuration
#
CONFIG_FS_FAT=y
CONFIG_FAT_LCNAMES=y
CONFIG_FAT_LFN=y
CONFIG_FAT_MAXFNAME=32
CONFIG_FS_NXFFS=n
CONFIG_FS_ROMFS=n

#
# Maintain legacy build behavior (revisit)
#

CONFIG_MMCSD=y
CONFIG_MMCSD_SPI=y
CONFIG_MMCSD_SDIO=y
CONFIG_MTD=y

#
# SPI-based MMC/SD driver
#
CONFIG_MMCSD_NSLOTS=1
CONFIG_MMCSD_READONLY=n
CONFIG_MMCSD_SPICLOCK=12500000

#
# Block driver buffering
#
CONFIG_FS_READAHEAD=n
CONFIG_FS_WRITEBUFFER=n

#
# STM32 SDIO-based MMC/SD driver
#
CONFIG_SDIO_DMA=n
#CONFIG_SDIO_PRI=128
#CONFIG_SDIO_DMAPRIO
#CONFIG_SDIO_WIDTH_D1_ONLY
CONFIG_MMCSD_MULTIBLOCK_DISABLE=y
CONFIG_MMCSD_MMCSUPPORT=n
CONFIG_MMCSD_HAVECARDDETECT=n

#
# TCP/IP and UDP support via uIP
#
CONFIG_NET=y
CONFIG_NET_NOINTS=n
CONFIG_NET_MULTIBUFFER=y
CONFIG_NET_IPv6=n
CONFIG_NSOCKET_DESCRIPTORS=10
CONFIG_NET_SOCKOPTS=y
CONFIG_NET_BUFSIZE=562
CONFIG_NET_TCP=y
CONFIG_NET_TCP_CONNS=40
#CONFIG_NET_TCP_READAHEAD_BUFSIZE
CONFIG_NET_NTCP_READAHEAD_BUFFERS=16
CONFIG_NET_TCPBACKLOG=y
CONFIG_NET_MAX_LISTENPORTS=40
CONFIG_NET_UDP=y
CONFIG_NET_UDP_CHECKSUMS=y
#CONFIG_NET_UDP_CONNS=10
CONFIG_NET_ICMP=y
CONFIG_NET_ICMP_PING=y
#CONFIG_NET_PINGADDRCONF=0
CONFIG_NET_STATISTICS=y
#CONFIG_NET_RECEIVE_WINDOW=
CONFIG_NET_BROADCAST=n
#CONFIG_NET_ARPTAB_SIZE=8
CONFIG_NET_ARP_IPIN=n
CONFIG_NET_MULTICAST=n

#
# UIP Network Utilities
#
CONFIG_NET_DHCP_LIGHT=n
CONFIG_NET_RESOLV_ENTRIES=4

#
# FTP Server
#
CONFIG_FTPD_CMDBUFFERSIZE=2048

#
# RTC Configuration
#
CONFIG_RTC=y
CONFIG_RTC_DATETIME=y
CONFIG_RTC_HIRES=n
CONFIG_RTC_FREQUENCY=1
CONFIG_RTC_ALARM=n

#
# Input device configuration
#
CONFIG_INPUT=n
CONFIG_INPUT_TSC2007=n

#
# STMPE811 input device configuration
#
# Prerequisites:  CONFIG_INPUT=y
# Other settings that effect the driver: CONFIG_DISABLE_POLL
#
CONFIG_INPUT_STMPE811=n
CONFIG_STMPE811_SPI=n
CONFIG_STMPE811_I2C=y
CONFIG_STMPE811_MULTIPLE=y
CONFIG_STMPE811_ACTIVELOW=y
CONFIG_STMPE811_EDGE=y
#CONFIG_STMPE811_NPOLLWAITERS
CONFIG_STMPE811_TSC_DISABLE=n
CONFIG_STMPE811_ADC_DISABLE=y
CONFIG_STMPE811_GPIO_DISABLE=y
CONFIG_STMPE811_GPIOINT_DISABLE=y
CONFIG_STMPE811_SWAPXY=y
CONFIG_STMPE811_TEMP_DISABLE=y
CONFIG_STMPE811_REGDEBUG=n
CONFIG_STMPE811_THRESHX=26
CONFIG_STMPE811_THRESHY=34

#
# STM32 USB OTG FS Device Configuration
#
CONFIG_USBDEV=n
CONFIG_USBDEV_ISOCHRONOUS=n
CONFIG_USBDEV_DUALSPEED=n
CONFIG_USBDEV_SELFPOWERED=y
CONFIG_USBDEV_REMOTEWAKEUP=n
CONFIG_USBDEV_MAXPOWER=100
CONFIG_USBDEV_TRACE=n
CONFIG_USBDEV_TRACE_NRECORDS=128

#
# STM32 USB OTG FS Host Configuration
#
CONFIG_USBHOST=n
#CONFIG_STM32_OTGFS_RXFIFO_SIZE
#CONFIG_STM32_OTGFS_NPTXFIFO_SIZE
#CONFIG_STM32_OTGFS_PTXFIFO_SIZE
#CONFIG_STM32_OTGFS_DESCSIZE
CONFIG_STM32_OTGFS_SOFINTR=n
CONFIG_STM32_USBHOST_REGDEBUG=n
CONFIG_STM32_USBHOST_PKTDUMP=n

#
# USB Serial Device Configuration
#
CONFIG_PL2303=n
CONFIG_PL2303_EPINTIN=1
CONFIG_PL2303_EPBULKOUT=2
CONFIG_PL2303_EPBULKIN=3
CONFIG_PL2303_NWRREQS=4
CONFIG_PL2303_NRDREQS=4
CONFIG_PL2303_VENDORID=0x067b
CONFIG_PL2303_PRODUCTID=0x2303
CONFIG_PL2303_VENDORSTR="Nuttx"
CONFIG_PL2303_PRODUCTSTR="USBdev Serial"
CONFIG_PL2303_RXBUFSIZE=512
CONFIG_PL2303_TXBUFSIZE=512

#
# USB Storage Device Configuration
#
CONFIG_USBMSC=n
CONFIG_USBMSC_EP0MAXPACKET=64
CONFIG_USBMSC_EPBULKOUT=2
CONFIG_USBMSC_EPBULKIN=5
CONFIG_USBMSC_NRDREQS=2
CONFIG_USBMSC_NWRREQS=2
CONFIG_USBMSC_BULKINREQLEN=256
CONFIG_USBMSC_BULKOUTREQLEN=256
CONFIG_USBMSC_VENDORID=0x584e
CONFIG_USBMSC_VENDORSTR="NuttX"
CONFIG_USBMSC_PRODUCTID=0x5342
CONFIG_USBMSC_PRODUCTSTR="USBdev Storage"
CONFIG_USBMSC_VERSIONNO=0x0399
CONFIG_USBMSC_REMOVABLE=y

#
# Graphics related configuration settings
#
CONFIG_NX=n
CONFIG_NX_MULTIUSER=n
CONFIG_NX_NPLANES=1
CONFIG_NX_DISABLE_1BPP=y
CONFIG_NX_DISABLE_2BPP=y
CONFIG_NX_DISABLE_4BPP=y
CONFIG_NX_DISABLE_8BPP=y
CONFIG_NX_DISABLE_16BPP=n
CONFIG_NX_DISABLE_24BPP=y
CONFIG_NX_DISABLE_32BPP=y
CONFIG_NX_PACKEDMSFIRST=n
CONFIG_NX_LCDDRIVER=y
CONFIG_LCD_MAXPOWER=1
CONFIG_LCD_MAXCONTRAST=1
CONFIG_NX_MOUSE=y
CONFIG_NX_KBD=y
#CONFIG_NXTK_BORDERWIDTH=4
CONFIG_NXTK_BORDERCOLOR1=0xd69a
CONFIG_NXTK_BORDERCOLOR2=0xad55
CONFIG_NXTK_AUTORAISE=n
CONFIG_NXFONT_SANS17X22=y
CONFIG_NXFONT_SANS20X26=n
CONFIG_NXFONT_SANS22X29=n
CONFIG_NXFONT_SANS23X27=n
CONFIG_NXFONT_SANS28X37=n
CONFIG_NXFONT_SANS17X23B=n
CONFIG_NXFONT_SANS20X27B=y
CONFIG_NXFONT_SANS22X29B=y
CONFIG_NXFONT_SANS28X37B=n
CONFIG_NXFONT_SANS40X49B=n
CONFIG_NXFONT_SERIF22X29=n
CONFIG_NXFONT_SERIF29X37=n
CONFIG_NXFONT_SERIF38X48=n
CONFIG_NXFONT_SERIF22X28B=n
CONFIG_NXFONT_SERIF27X38B=n
CONFIG_NXFONT_SERIF38X49B=n
CONFIG_NXFONTS_CHARBITS=7
CONFIG_NX_BLOCKING=y
CONFIG_NX_MXSERVERMSGS=32
CONFIG_NX_MXCLIENTMSGS=16

#
# NxConsole Configuration Settings:
#
CONFIG_NXCONSOLE=n
CONFIG_NXCONSOLE_BPP=16
CONFIG_NXCONSOLE_MXCHARS=256
CONFIG_NXCONSOLE_CACHESIZE=32
#

#
# STM3240G-EVAL LCD Hardware Configuration
#
CONFIG_LCD_NOGETRUN=y
CONFIG_LCD_LANDSCAPE=n
CONFIG_LCD_RLANDSCAPE=n
CONFIG_LCD_PORTRAIT=n
CONFIG_LCD_RPORTRAIT=y

#
# STM3240G-EVAL specific LCD settings
#
CONFIG_STM32_ILI9320_DISABLE=n
CONFIG_STM32_ILI9325_DISABLE=n

#
# Settings for examples/uip
#
CONFIG_EXAMPLES_UIP_IPADDR=0x0a000002
CONFIG_EXAMPLES_UIP_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_UIP_NETMASK=0xffffff00
CONFIG_EXAMPLES_UIP_DHCPC=n

#
# Settings for examples/nettest
CONFIG_EXAMPLES_NETTEST_SERVER=n
CONFIG_EXAMPLES_NETTEST_PERFORMANCE=n
CONFIG_EXAMPLES_NETTEST_NOMAC=y
CONFIG_EXAMPLES_NETTEST_IPADDR=0x0a000002
CONFIG_EXAMPLES_NETTEST_DRIPADDR=0x0a000001
CONFIG_EXAMPLES_NETTEST_NETMASK=0xffffff00
CONFIG_EXAMPLES_NETTEST_CLIENTIP=0x0a000001

#
# Settings for examples/ostest
#
CONFIG_EXAMPLES_OSTEST_LOOPS=1
CONFIG_EXAMPLES_OSTEST_STACKSIZE=2048
CONFIG_EXAMPLES_OSTEST_NBARRIER_THREADS=3

#
# Settings for apps/nshlib
#
CONFIG_BUILTIN=y
CONFIG_NSH_BUILTIN_APPS=y
CONFIG_NSH_FILEIOSIZE=512
CONFIG_NSH_STRERROR=n
CONFIG_NSH_LINELEN=64
CONFIG_NSH_NESTDEPTH=3
CONFIG_NSH_DISABLESCRIPT=n
CONFIG_NSH_DISABLEBG=n
CONFIG_NSH_ROMFSETC=n
CONFIG_NSH_CONSOLE=y
CONFIG_NSH_TELNET=y
CONFIG_NSH_ARCHINIT=n
CONFIG_NSH_IOBUFFER_SIZE=512
CONFIG_NSH_DHCPC=n
CONFIG_NSH_NOMAC=y
CONFIG_NSH_IPADDR=0x0a000002
CONFIG_NSH_DRIPADDR=0x0a000001
CONFIG_NSH_NETMASK=0xffffff00
CONFIG_NSH_ROMFSMOUNTPT="/etc"
CONFIG_NSH_INITSCRIPT="init.d/rcS"
CONFIG_NSH_ROMFSDEVNO=0
CONFIG_NSH_ROMFSSECTSIZE=64
CONFIG_NSH_FATDEVNO=1
CONFIG_NSH_FATSECTSIZE=512
CONFIG_NSH_FATNSECTORS=1024
CONFIG_NSH_FATMOUNTPT="/tmp"

#
# Architecture-specific NSH options
#
CONFIG_NSH_MMCSDSPIPORTNO=0
CONFIG_NSH_MMCSDSLOTNO=0
CONFIG_NSH_MMCSDMINOR=0

#
# I2C tool settings
#
CONFIG_I2CTOOL_MINBUS=1
CONFIG_I2CTOOL_MAXBUS=3
#CONFIG_I2CTOOL_MINADDR
#CONFIG_I2CTOOL_MAXADDR
#CONFIG_I2CTOOL_MAXREGADDR
CONFIG_I2CTOOL_DEFFREQ=100000

#
# Settings for examples/usbserial
#
CONFIG_EXAMPLES_USBSERIAL_INONLY=n
CONFIG_EXAMPLES_USBSERIAL_OUTONLY=n
CONFIG_EXAMPLES_USBSERIAL_ONLYSMALL=n
CONFIG_EXAMPLES_USBSERIAL_ONLYBIG=n

CONFIG_EXAMPLES_USBSERIAL_TRACEINIT=n
CONFIG_EXAMPLES_USBSERIAL_TRACECLASS=n
CONFIG_EXAMPLES_USBSERIAL_TRACETRANSFERS=n
CONFIG_EXAMPLES_USBSERIAL_TRACECONTROLLER=n
CONFIG_EXAMPLES_USBSERIAL_TRACEINTERRUPTS=n

#
# Settings for examples/adc
#

#
# Settings for examples/can
#

#
# Settings for examples/nx
#
CONFIG_EXAMPLES_NX_VPLANE=0
CONFIG_EXAMPLES_NX_DEVNO=0
CONFIG_EXAMPLES_NX_BGCOLOR=0x0011
CONFIG_EXAMPLES_NX_COLOR1=0xaedc
CONFIG_EXAMPLES_NX_COLOR2=0xe7ff
CONFIG_EXAMPLES_NX_TBCOLOR=0xd69a
CONFIG_EXAMPLES_NX_FONTID=0
CONFIG_EXAMPLES_NX_FONTCOLOR=0x0000
CONFIG_EXAMPLES_NX_BPP=16
CONFIG_EXAMPLES_NX_RAWWINDOWS=n
CONFIG_EXAMPLES_NX_STACKSIZE=2048
CONFIG_EXAMPLES_NX_CLIENTPRIO=80
CONFIG_EXAMPLES_NX_SERVERPRIO=120
CONFIG_EXAMPLES_NX_NOTIFYSIGNO=4
CONFIG_EXAMPLES_NX_EXTERNINIT=n

#
# Settings for examples/nxhello
#
CONFIG_EXAMPLES_NXHELLO_VPLANE=0
CONFIG_EXAMPLES_NXHELLO_DEVNO=0
CONFIG_EXAMPLES_NXHELLO_BGCOLOR=0x0011
CONFIG_EXAMPLES_NXHELLO_FONTID=6
CONFIG_EXAMPLES_NXHELLO_FONTCOLOR=0xffdf
CONFIG_EXAMPLES_NXHELLO_BPP=16
CONFIG_EXAMPLES_NXHELLO_EXTERNINIT=n

#
# Settings for examples/nximage
#
CONFIG_EXAMPLES_NXIMAGE_VPLANE=0
CONFIG_EXAMPLES_NXIMAGE_DEVNO=0
CONFIG_EXAMPLES_NXIMAGE_BPP=16
CONFIG_EXAMPLES_NXIMAGE_XSCALEp5=n
CONFIG_EXAMPLES_NXIMAGE_XSCALE1p5=y
CONFIG_EXAMPLES_NXIMAGE_XSCALE2p0=n
CONFIG_EXAMPLES_NXIMAGE_YSCALEp5=n
CONFIG_EXAMPLES_NXIMAGE_YSCALE1p5=y
CONFIG_EXAMPLES_NXIMAGE_YSCALE2p0=n
CONFIG_EXAMPLES_NXIMAGE_EXTERNINIT=n

#
# Settings for examples/nxlines
#
CONFIG_EXAMPLES_NXLINES_VPLANE=0
CONFIG_EXAMPLES_NXLINES_DEVNO=0
CONFIG_EXAMPLES_NXLINES_BGCOLOR=0x0320
CONFIG_EXAMPLES_NXLINES_LINEWIDTH=16
CONFIG_EXAMPLES_NXLINES_LINECOLOR=0xffe0
CONFIG_EXAMPLES_NXLINES_BORDERWIDTH=4
CONFIG_EXAMPLES_NXLINES_BORDERCOLOR=0xffe0
CONFIG_EXAMPLES_NXLINES_CIRCLECOLOR=0xf7bb
CONFIG_EXAMPLES_NXLINES_BPP=16
CONFIG_EXAMPLES_NXLINES_EXTERNINIT=n

#
# Settings for examples/touchscreen
#
CONFIG_EXAMPLES_TOUCHSCREEN_MINOR=0
CONFIG_EXAMPLES_TOUCHSCREEN_DEVPATH="/dev/input0"
CONFIG_EXAMPLES_TOUCHSCREEN_NSAMPLES=25

#
# Settings for examples/usbstorage
#
CONFIG_EXAMPLES_USBMSC_NLUNS=1
CONFIG_EXAMPLES_USBMSC_DEVMINOR1=0
CONFIG_EXAMPLES_USBMSC_DEVPATH1="/dev/mmcsd0"
CONFIG_EXAMPLES_USBMSC_DEBUGMM=n
CONFIG_EXAMPLES_USBMSC_TRACEINIT=n
CONFIG_EXAMPLES_USBMSC_TRACECLASS=n
CONFIG_EXAMPLES_USBMSC_TRACETRANSFERS=n
CONFIG_EXAMPLES_USBMSC_TRACECONTROLLER=n
CONFIG_EXAMPLES_USBMSC_TRACEINTERRUPTS=n

#
# Settings for examples/watchdog
#
# This test depends on these specific Watchdog/NSH configurations settings (your
# specific watchdog hardware settings might require additional settings).
#

#
# Settings for examples/pwm
#

#
# Settings for examples/ftpd
#

#
# Stack and heap information
#
CONFIG_BOOT_RUNFROMFLASH=n
CONFIG_BOOT_COPYTORAM=n
CONFIG_CUSTOM_STACK=n
CONFIG_IDLETHREAD_STACKSIZE=1024
CONFIG_USERMAIN_STACKSIZE=2048
CONFIG_PTHREAD_STACK_MIN=256
CONFIG_PTHREAD_STACK_DEFAULT=2048
