############################################################################
# arch/arm/src/lpc43xx/Make.defs
#
#   Copyright (C) 2012-2013 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################

HEAD_ASRC  =

CMN_ASRCS  = up_saveusercontext.S up_fullcontextrestore.S up_switchcontext.S
CMN_ASRCS += vfork.S

CMN_CSRCS  = up_assert.c up_blocktask.c up_copystate.c
CMN_CSRCS += up_createstack.c up_mdelay.c up_udelay.c up_exit.c
CMN_CSRCS += up_initialize.c up_initialstate.c up_interruptcontext.c
CMN_CSRCS += up_memfault.c up_modifyreg8.c up_modifyreg16.c up_modifyreg32.c
CMN_CSRCS += up_releasepending.c up_releasestack.c up_reprioritizertr.c
CMN_CSRCS += up_schedulesigaction.c up_sigdeliver.c up_unblocktask.c
CMN_CSRCS += up_usestack.c up_doirq.c up_hardfault.c up_svcall.c up_vfork.c

ifeq ($(CONFIG_ARMV7M_CMNVECTOR),y)
CMN_ASRCS += up_exception.S
CMN_CSRCS += up_vectors.c
endif

ifeq ($(CONFIG_ARCH_RAMVECTORS),y)
CMN_CSRCS += up_ramvec_initialize.c up_ramvec_attach.c
endif

ifeq ($(CONFIG_ARCH_MEMCPY),y)
CMN_ASRCS += up_memcpy.S
endif

ifeq ($(CONFIG_NUTTX_KERNEL),y)
CMN_CSRCS += up_mpu.c up_task_start.c up_pthread_start.c up_stackframe.c
ifneq ($(CONFIG_DISABLE_SIGNALS),y)
CMN_CSRCS += up_signal_dispatch.c
CMN_UASRCS += up_signal_handler.S
endif
endif

ifeq ($(CONFIG_DEBUG_STACK),y)
CMN_CSRCS += up_checkstack.c
endif

ifeq ($(CONFIG_ELF),y)
CMN_CSRCS += up_elf.c
endif

ifeq ($(CONFIG_ARCH_FPU),y)
CMN_ASRCS += up_fpu.S
endif

CHIP_ASRCS  = 
CHIP_CSRCS  = lpc43_allocateheap.c lpc43_cgu.c lpc43_clrpend.c lpc43_gpio.c
CHIP_CSRCS += lpc43_irq.c lpc43_pinconfig.c lpc43_rgu.c lpc43_serial.c
CHIP_CSRCS += lpc43_start.c lpc43_timerisr.c lpc43_uart.c

ifeq ($(CONFIG_NUTTX_KERNEL),y)
CHIP_CSRCS += lpc43_userspace.c lpc43_mpuinit.c
endif

ifneq ($(CONFIG_IDLE_CUSTOM),y)
CHIP_CSRCS += lpc43_idle.c
endif

ifeq ($(CONFIG_DEBUG),y)
CHIP_CSRCS += lpc43_debug.c
endif

ifeq ($(CONFIG_LPC43_GPDMA),y)
CHIP_CSRCS += lpc43_gpdma.c
endif

ifeq ($(CONFIG_GPIO_IRQ),y)
CHIP_CSRCS += lpc43_gpioint.c
endif

ifeq ($(CONFIG_LPC43_SPI),y)
CHIP_CSRCS += lpc43_spi.c
endif

ifeq ($(CONFIG_LPC43_SPIFI),y)
CHIP_CSRCS += lpc43_spifi.c
endif

ifeq ($(CONFIG_LPC43_SSP0),y)
CHIP_CSRCS += lpc43_ssp.c
else
ifeq ($(CONFIG_LPC43_SSP1),y)
CHIP_CSRCS += lpc43_ssp.c
endif
endif

ifeq ($(CONFIG_LPC43_I2C0),y)
CHIP_CSRCS += lpc43_i2c.c
else
ifeq ($(CONFIG_LPC43_I2C1),y)
CHIP_CSRCS += lpc43_i2c.c
endif
endif

ifeq ($(CONFIG_LPC43_ADC0),y)
CHIP_CSRCS += lpc43_acc.c
else
ifeq ($(CONFIG_LPC43_ADC1),y)
CHIP_CSRCS += lpc43_adc.c
endif
endif

ifeq ($(CONFIG_LPC43_DAC),y)
CHIP_CSRCS += lpc43_acc.c
else
ifeq ($(CONFIG_LPC43_DAC),y)
CHIP_CSRCS += lpc43_adc.c
endif
endif

ifeq ($(CONFIG_LPC43_USB0),y)
ifeq ($(CONFIG_USBDEV),y)
CHIP_CSRCS	+= lpc31_usb0dev.c
endif
endif

